## Uses of Class
com.hazelcast.config.IcmpFailureDetectorConfig

- Packages that use IcmpFailureDetectorConfig
  Package | Description
  --- | ---
  com.hazelcast.config | Provides classes for configuring HazelcastInstance.

- - ### Uses of IcmpFailureDetectorConfig in com.hazelcast.config

    Methods in com.hazelcast.config that return IcmpFailureDetectorConfig
    Modifier and Type | Method and Description
    --- | ---
    `IcmpFailureDetectorConfig` | NetworkConfig.`getIcmpFailureDetectorConfig()` Returns the current `IcmpFailureDetectorConfig`.
    `IcmpFailureDetectorConfig` | AdvancedNetworkConfig.`getIcmpFailureDetectorConfig()` Returns the current `IcmpFailureDetectorConfig`.
    `IcmpFailureDetectorConfig` | AdvancedNetworkConfig.MemberNetworkingView.`getIcmpFailureDetectorConfig()`
    `IcmpFailureDetectorConfig` | IcmpFailureDetectorConfig.`setEnabled(boolean enabled)` Set whether the ICMP failure detector should be enabled or not.
    `IcmpFailureDetectorConfig` | IcmpFailureDetectorConfig.`setFailFastOnStartup(boolean failFastOnStartup)` Sets whether the member should fail-fast on startup if ICMP is not allowed by the underlying OS.
    `IcmpFailureDetectorConfig` | IcmpFailureDetectorConfig.`setIntervalMilliseconds(int intervalMilliseconds)` Sets the time in milliseconds between each ping This value can not be smaller than 1000 milliseconds
    `IcmpFailureDetectorConfig` | IcmpFailureDetectorConfig.`setMaxAttempts(int maxAttempts)` Set the max ping attempts before suspecting a member
    `IcmpFailureDetectorConfig` | IcmpFailureDetectorConfig.`setParallelMode(boolean mode)` Set the ICMP detector to run in parallel mode, independent from the other failure detectors.
    `IcmpFailureDetectorConfig` | IcmpFailureDetectorConfig.`setTimeoutMilliseconds(int timeoutMilliseconds)` Sets the timeout in Milliseconds before declaring a failed ping This cannot be more than the interval value.
    `IcmpFailureDetectorConfig` | IcmpFailureDetectorConfig.`setTtl(int ttl)` Sets the maximum number of times the IP Datagram (ping) can be forwarded, in most cases all Hazelcast cluster members would be within one network switch/router therefore

    Methods in com.hazelcast.config with parameters of type IcmpFailureDetectorConfig
    Modifier and Type | Method and Description
    --- | ---
    `NetworkConfig` | NetworkConfig.`setIcmpFailureDetectorConfig(IcmpFailureDetectorConfig icmpFailureDetectorConfig)` Sets the `IcmpFailureDetectorConfig`.
    `AdvancedNetworkConfig` | AdvancedNetworkConfig.`setIcmpFailureDetectorConfig(IcmpFailureDetectorConfig icmpFailureDetectorConfig)` Sets the `IcmpFailureDetectorConfig`.
    `NetworkConfig` | AdvancedNetworkConfig.MemberNetworkingView.`setIcmpFailureDetectorConfig(IcmpFailureDetectorConfig icmpFailureDetectorConfig)`

Copyright © 2020. All rights reserved.